**Using an Interactive Board on the Mac Side**

1. If necessary, plug in board to the USB port.
2. If you are using a promethean board, go to your apps folder and click on interactive white boards.
3. Select Activ board settings and click on calibrate.
4. Hit the cross hairs to orient the board.
5. If using a polyvision board, click on your hard drive.
6. Click on Polyvision Driver
7. An icon- it looks like a white board- will appear up on the menu bar.
8. Click on the icon and select Configure Polyvison Driver.
9. Your pen should appear in the window. Click on it once and then click OK.
10. Touch your board with your pen. It will turn green.
11. Touch the cross hairs with your pen to orient the board.